Approved by the order of the Chairman of Azerbaijan Caspian Shipping Closed Joint Stock Company dated 1st of December 2016No. 216.



**AZERBAIJAN CASPIAN SHIPPING CLOSED JOINT STOCK COMPANY**

**IS ANNOUNCING OPENBIDDING FOR THE PROCUREMENT OF SERVICES RELATING TO THE INSTALLATION OF HEATING SYSTEM OF THE MULTI STOREYED RESIDENTIAL BUILDING OF "DENIZCHI" HOUSING CONSTRUCTION COOPERATIVE WITH A KINDERGARTEN ON THE GROUND FLOOR**

**B I D D I N G No. AM077/2021**

|  |  |
| --- | --- |
|  | **Submission documentation required for participation in the bidding :**   * Application for participation in the bidding (template has been attached hereto) ; * Bank evidence as a proof of participation fee ; * Bidding offer : * Bank document confirming financial condition of the consignor within the last year (or within the period of operation if less than one year) ; * Statement issued by the relevant tax authorities on the absence of expired commitments associated with taxes and other compulsory payments and failure of obligations set forth in the Tax Code of the Republic of Azerbaijan for the last one year (excluding the period of suspension).   At the initial stage, application for participation in the bidding ( signed and stamped ) and bank evidence proving payment of participation fee (excluding bidding offer) shall be submitted in English, Russian or in Azerbaijani to the official address of Azerbaijan Caspian Shipping CJSC (hereinafter referred to as "ASCO" or "Procuring Organization") through email address of contact person in charge by **17.00** (Baku time) on **November 12, 2021**. Whereas, other necessary documents shall be submitted as enclosed in the bidding offer envelope.    Description (list) of goods, works or services has been attached hereto. |
|  | **The participation fee and Collection of General Terms and Conditions:**   * Any participant (bidder), who desires to participate in the bidding, shall pay for participation fee stated below (the payment order shall necessarily state the name of the organization holding open bidding and the subject of the bidding) and shall submit the evidence as a proof of payment to ASCO not later than the date stipulated in section one. All participants (bidders), who have fulfilled these requirements, may obtain General Terms and Conditions relating to the procurement subject from contact person in charge by the date envisaged in section IV of this announcement at any time from 09.00 till 18.00 in any business day of the week. * Participation fee amount (VAT exclusive): AZN 250 * The participation fee may be paid in AZN or equivalent amount thereof in USD or EURO. * ***Account No. :***  |  |  |  | | --- | --- | --- | | A Z N | U S D | E U R O | | Name : The International Bank of Azerbaijan  ABB- Customer Service Department  Code : 805250  TAX ID : 9900001881  Correspondent account : AZ03NABZ01350100000000002944  SWIFT : IBAZAZ2X  Beneficiary : AZARB.XAZAR DANIZ GAMICILIYI QSC  TAX ID : 1701579951  Account No. (AZN) : AZ36IBAZ38050019441115341120 | Intermediary Bank : Citibank N.Y,  New York  Acc.36083186, SWIFT: CITIUS33  Beneficiary Bank : The International Bank of Azerbaijan  IBA- Customer Service Department  SWIFT : IBAZAZ2X  Nizami str., 67 Beneficiary : AZARB.XAZAR DANIZ GAMICILIYI QSC  TAX ID : 1701579951  Account No. : AZ26IBAZ38150018401115341120 | Intermediary Bank : Commerzbank AG, Frankfurt am Main  SWIFT : COBADEFF  ACC # 400 88 660 3001  Beneficiary Bank : The International Bank of Azerbaijan,  IBA-Premier Customer Service SWIFT : IBAZAZ2X Nizami str., 67 Beneficiary : Azerbaijan Caspian Shipping CJSC  TAX ID : 1701579951  Account No. : AZ06IBAZ38150019781115341120 |  * **Except for circumstances where the bidding is cancelled by ASCO, participation fee shall in no case be refunded !** |
|  | **Security for a bidding offer :**   * The bank guarantee is required in the amount of at least 1 (one) % of the bidding offer price. A bank guarantee sample shall be specified in the General Terms and Conditions. * Bank guarantees shall be submitted as enclosed in the bidding offer envelope along with the bidding offer. Otherwise, the Purchasing Organization shall reserve the right to reject such offer. * The financial institution that issued the guarantee should be acknowledged in the Republic of Azerbaijan and / or international financial transactions. The purchasing organization shall reserve the right not to accept and reject any unreliable bank guarantee. * Persons wishing to participate in the bidding and intending to submit another type of warranty (letter of credit, securities, transfer of funds to the special banking account set forth by the Procuring Organization in the bidding documents, deposit and other financial assets) shall request and obtain a consent from ASCO through the contact person reflected in the announcement on the acceptability of such type of warranty. * Contract performance bond is required in the amount of 5 (five) % of the purchase price. |
|  | **Final deadline date and time for submission of the bidding offer :**   * All participants, which have submitted their application for participation in the bidding and bank evidence as a proof of payment of participation fee by the date and time stipulated in section one, and shall submit their bidding offer (one original and two copies) enclosed in sealed envelope to ASCO by **17.00** Baku time on **November 18, 2021**. * All bidding offer envelopes submitted after above-mentioned date and time shall be returned back unopened. |
|  | **Address of the procuring company :**  Republic of Azerbaijan, AZ1003, Baku city, 2 Neftchilar avenue , ASCO Procurement Committee.  .  **Contact person in charge:**  Emil Hasanov  Senior procurement specialist at the Procurement Department of ASCO  Telephone No. : +99450 422 00 11  E-mail: emil.hasanov@asco.az, [tender@asco.az](mailto:tender@asco.az)  **Zaur Salamov**  Procurement specialist at the Procurement Department of ASCO  **Telephone No.: +99455 817 08 12**  E-mail: zaur.salamov@asco.az  **Contact person on legal issues :**  Landline No.: +994 12 4043700 (ext: 1262)  Email address[:](mailto:tender@asco.az) tender@asco.az |
|  | **Date and time assigned for the opening of bidding offer envelopes:**  Opening of the envelopes shall take place on **November 19, 2021** at **15.00** Baku time in the address stated in section V of the announcement.  Persons wishing to participate in the opening of the envelopes shall submit a document confirming their permission to participate (the relevant power of attorney from the participating legal entity or natural person) and the ID card at least half an hour before the commencement of the bidding. |
|  | **Information on the winner of the bidding :**  Information on the winner of the bidding will be posted in the "Announcements" section of the ASCO official website. |

(On the participant`s letter head)

APPLICATION FOR PARTICIPATION IN

THE OPEN BIDDING

\_\_\_\_\_\_\_\_\_\_\_ city “\_\_”\_\_\_\_\_\_\_20\_

\_\_\_\_\_\_\_\_\_\_\_№

To the attention of the Chairman of ASCO Procurement Committee

Mr Jabrail Mahmudlu

We, hereby confirm the intention of [ to state full name of the participant ] to participate in the open bidding No. [ bidding No. shall be inserted by participant ] announced by ASCO in respect of procurement of "\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_" .

Moreover, we confirm that no winding - up or bankruptcy proceeding is being performed or there is no circumstance of cessation of activities or any other circumstance that may impede participation of [ to state full name of the participant ] in the stated bidding.

In addition, we warrant that [ to state full name of the participant ] is not an affiliate of ASCO.

Below mentioned contact details are available to respond to any question that may emerge in relation to the documents submitted and other issues :

* Contact person in charge : . . . . . . . . . . . . . . . . . . . . . . .
* Position of the contact person : . . . . . . . . . . . . . . . . . . . . . . .
* Telephone No. : . . . . . . . . . . . . . . . . . . . . . . .
* E-mail: . . . . . . . . . . . . . . . . . . . . . . .

Attachment :

1. Original of the bank evidence as a proof of payment of participation fee – \_\_ page(s).

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(initials of the authorized person) (signature of the authorized person)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(position of the authorized person)

**LIST OF THE GOODS :**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item No.** | **Materials, description of works** | **Measurement unit** | **Total** | **Certification requirement** |
| **"1A" - heating system** | | | | |
|  | Installation of steel electric welded pipe ∅ 76 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 57 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 48 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 40 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 64 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅25 х 2,3 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 3520 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅20 х 1,9 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 5712 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅100 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 6 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅70 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅50 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅40 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅32 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 64 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅25 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 3520 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅20 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 5712 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 18 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 2 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 16 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 26 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 15 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 41 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 14 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 20 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 13 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 1 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 12 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 4 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 11 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 47 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 10 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 32 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 9 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 39 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 8 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 8 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 7 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 29 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 6 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 89 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators (inclusive of materials) Sections = 5 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 | pcs | 56 | Certificate of conformity and quality |
|  | Installation of brass radiator valve (inclusive of materials) ∅15 PN10 / ЛС59-1 ГОСТ 15527-2004 | pcs | 788 | Certificate of conformity and quality |
|  | Installation of radiator acessories (radiator hanging hook 2 pcs, radiator headings 4 pcs, bleeder screw 1 pc, ∅15 connector - outer thread - 2 pcs for each set) (inclusive of materials) | set | 394 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.)∅32, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 32 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve (inclusive of materials) ∅20, SDR6 PN10 ГОСТ 32415-2013 | pcs | 180 | Certificate of conformity and quality |
|  | Installation of brass dynamic balancing valve (inclusive of materials) ∅32, 0-120 ºC, serrated joint, brass, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 90 | Certificate of conformity and quality |
|  | Installation of air release valve ∅20, 0-120 ºC, serrated joint, brass, PN10 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Installation of collecting pipe made of ∅32 electric welded steel pipe (with 6 outlets - outlet ∅25 ) (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
|  | Installation of cast iron sludge trap (dirt collector); ∅32, PN16 (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
| **Control junction 1, 2, 3, 4, 5 (inclusive of materials)** | | | | |
|  | Installation of steel electric welded pipe ∅ 108 x 4 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 6 | Certificate of conformity and quality |
|  | Galvanized steel pipe for hot water supply ∅65 x 3,2 mm ГОСТ 3262-75 (with piping components - flare joint, elbow pipe etc.) (inclusive of materials) | metre | 6 | Certificate of conformity and quality |
|  | Galvanized steel pipe for hot water supply ∅40 x 3,0 mm ГОСТ 3262-75 (with piping components - flare joint, elbow pipe etc.) (inclusive of materials) | metre | 9 | Certificate of conformity and quality |
|  | Galvanized steel pipe for hot water supply ∅20 x 2,5 mm ГОСТ 3262-75 (with piping components - flare joint, elbow pipe etc.) (inclusive of materials) | metre | 3 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.)∅100, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 8 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.)∅50, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.) ∅ 65, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 4 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.) ∅ 40, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 6 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.) ∅ 32, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.) ∅ 25, PN10 / ЛС59-1 ГОСТ 15527-2004 | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.) ∅ 20, PN10 / ЛС59-1 ГОСТ 15527-2004 | pcs | 4 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.) ∅ 15, PN10 / ЛС59-1 ГОСТ 15527-2004 | pcs | 6 | Certificate of conformity and quality |
|  | Installation of cast iron sludge trap (dirt collector); ∅100, PN16 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Installation of cast iron sludge trap (dirt collector); ∅65, PN16 (inclusive of materials) | pcs | 3 | Certificate of conformity and quality |
|  | Installation of cast iron sludge trap (dirt collector); ∅40, PN16 (inclusive of materials) | pcs | 3 | Certificate of conformity and quality |
|  | Installation of cast iron sludge trap (dirt collector); ∅ 25, PN10 (inclusive of materials) | pcs | 1 | Certificate of conformity and quality |
|  | Installation of pressure regulating industrial pressure gauge (monometer) D - Ø100; thread - m 20 x 1,5; accuracy class - 2,5; 16 bar; İP-40; vibration resistant ГОСТ 2405-88 0-6 bar, (inclusive of materials) | pcs | 20 | Certificate of conformity and quality |
|  | Installation of technical temperature gauge 0-120 ºC, Alltan joint, Brass, Bi-Metallic, Ø 100 mm (inclusive of materials) | pcs | 10 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅159 х 4,0 / l=2000 mm (outlet - 40 x 3 mm -1 pc., 57 x 3,0 mm - 1 pc, 108 x 3 mm - 1 pc) (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
| **"1B" - heating system** | | | | |
|  | Installation of steel electric welded pipe ∅ 76 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 57 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 48 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 40 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 64 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅25 х 2,3 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 3520 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅20 х 1,9 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 5712 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅70 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅50 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅40 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅32 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 64 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅25 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 3520 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅20 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 5712 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 18 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 16 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 26 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 15 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 42 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 14 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 20 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 12 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 11 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 47 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 10 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 3 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 9 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 53 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 8 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 23 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 7 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 29 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 6 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 89 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 5 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 56 | Certificate of conformity and quality |
|  | Installation of brass radiator valve ∅15 PN10 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 788 | Certificate of conformity and quality |
|  | Installation of radiator accessories (radiator hanging hook 2 pcs, radiator headings 4 pcs, bleeder screw 1 pc, ∅15 connector - outer thread - 2 pcs for each set) (inclusive of materials) | set | 394 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve ∅25, SDR6 PN10 ГОСТ 32415-2013 (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve ∅20, SDR6 PN10 ГОСТ 32415-2013 (inclusive of materials) | pcs | 180 | Certificate of conformity and quality |
|  | Installation of brass dynamic balancing valve ∅32, 0-120 ºC, serrated joint, brass, PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 90 | Certificate of conformity and quality |
|  | Installation of air release valve ∅20, 0-120 ºC, serrated joint, brass, PN10 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Installation of collecting pipe made of ∅25 electric welded steel pipe (with 7 outlets - outlet ∅25 ) (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
|  | Installation of plastic sludge trap (dirt collector); ∅ 25, PN10 (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
| **"1C" - heating system** | | | | |
|  | Installation of steel electric welded pipe ∅ 76 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 57 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 48 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 40 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 64 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅70 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅50 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅40 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅32 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 64 | Certificate of conformity and quality |
|  | Installation of collecting pipe made of ∅32 electric welded steel pipe (with 6 outlets - outlet ∅25 ) (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
|  | Installation of plastic sludge trap (dirt collector); ∅ 25, PN10 (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
| **Kindergarten 1A, 1B, 1C - heating system** | | | | |
|  | Installation of steel electric welded pipe ∅ 57 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 12 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 48 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 28 | Certificate of conformity and quality |
| 1. 2 | Installation of steel electric welded pipe ∅ 40 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 118 | Certificate of conformity and quality |
| 1. 3 | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅32 х 2,9 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 155 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅25 х 2,3 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 365 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅20 х 1,9 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 583 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅50 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 12 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅40 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 28 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅32 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 273 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅25 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 365 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅20 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 583 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 14 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 16 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 13 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 10 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 12 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 11 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 12 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 10 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 7 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 9 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 5 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 8 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 14 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 6 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 3 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 5 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 12 | Certificate of conformity and quality |
|  | Installation of brass radiator valve (inclusive of materials) ∅15 PN10 / ЛС59-1 ГОСТ 15527-2004 | pcs | 162 | Certificate of conformity and quality |
|  | Installation of radiator accessories (radiator hanging hook 2 pcs, radiator headings 4 pcs, bleeder screw 1 pc, ∅15 connector - outer thread - 2 pcs for each set) (inclusive of materials) | set | 81 | Certificate of conformity and quality |
|  | Installation of brass radiator valve (inclusive of materials) ∅32 PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 10 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve ∅20, SDR6 PN10 ГОСТ 32415-2013 (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
|  | Installation of brass dynamic balancing valve ∅32, 0-120 ºC, serrated joint, brass, PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 15 | Certificate of conformity and quality |
|  | Installation of collecting pipe made of ∅32 electric welded steel pipe (with 7 outlets - outlet ∅25 ) (inclusive of materials) | pcs | 5 | Certificate of conformity and quality |
|  | Installation of plastic sludge trap (dirt collector); ∅ 32, PN16 (inclusive of materials) | pcs | 5 | Certificate of conformity and quality |
| **"2A" - heating system** | | | | |
|  | Installation of steel electric welded pipe ∅ 76 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 57 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 48 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 40 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 64 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅25 х 2,3 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 3520 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅20 х 1,9 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 5712 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅70 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅50 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | m | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅40 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | m | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅32 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | m | 64 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅25 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | m | 3520 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅20 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | m | 5712 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 18 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 17 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 16 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 15 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 54 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 14 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 13 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 6 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 12 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 28 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 11 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 14 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 10 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 58 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 9 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 8 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 23 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 7 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 37 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 6 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 106 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 5 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 70 | Certificate of conformity and quality |
|  | Installation of brass radiator valve ∅15 PN10 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 872 | Certificate of conformity and quality |
|  | Installation of radiator accessories (radiator hanging hook 2 pcs, radiator headings 4 pcs, bleeder screw 1 pc, ∅15 connector - outer thread - 2 pcs for each set) (inclusive of materials) | set | 436 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.) ∅ 80, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.) ∅ 70, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 2 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve ∅25, SDR6 PN10 ГОСТ 32415-2013 (inclusive of materials) | pcs | 32 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve ∅20, SDR6 PN10 ГОСТ 32415-2013 (inclusive of materials) | pcs | 224 | Certificate of conformity and quality |
|  | Installation of brass dynamic balancing valve ∅25, 0-120 ºC, serrated joint, brass, PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 112 | Certificate of conformity and quality |
|  | Installation of air release valve ∅20, 0-120 ºC, serrated joint, brass, PN10 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Installation of ∅ 32 electric welded steel collecting pipe (with 7 outlets) (inclusive of materials) | pcs | 32 | Certificate of conformity and quality |
|  | Installation of plastic sludge trap (dirt collector); ∅ 32, PN16 (inclusive of materials) | pcs | 32 | Certificate of conformity and quality |
| **"2B" - heating system** | | | | |
|  | Installation of steel electric welded pipe ∅ 76 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 57 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 48 x 2,5 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 40 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 64 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅25 х 2,3 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 3520 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅20 х 1,9 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 5712 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅70 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 136 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅50 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅40 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 16 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅32 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 64 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅25 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 3520 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅20 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 5712 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 18 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 16 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 15 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 49 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 14 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 15 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 13 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 1 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 12 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 11 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 47 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 10 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 18 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 9 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 47 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 8 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 21 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 7 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 6 h = 577mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 90 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 5 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 56 | Certificate of conformity and quality |
|  | Installation of brass radiator valve ∅15 PN10 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 820 | Certificate of conformity and quality |
|  | Installation of radiator accessories (radiator hanging hook 2 pcs, radiator headings 4 pcs, bleeder screw 1 pc, ∅15 connector - outer thread - 2 pcs for each set) (inclusive of materials) | set | 410 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve (with piping components - flare joint, elbow pipe etc.) ∅ 80, PN16 / ЛС59-1 ГОСТ 15527-2004 . (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve; (with piping components - flare joint, elbow pipe etc.) ∅ 70, PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve; (with piping components - flare joint, elbow pipe etc.) ∅ 50, PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass radiator valve (inclusive of materials) ∅40 PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 2 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve ∅25, SDR6 PN10 ГОСТ 32415-2013 (inclusive of materials) | pcs | 34 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve ∅20, SDR6 PN10 ГОСТ 32415-2013 (inclusive of materials) | pcs | 192 | Certificate of conformity and quality |
|  | Installation of brass dynamic balancing valve ∅25, 0-120 ºC, serrated joint, brass, PN16 / ЛС59-1 ГОСТ 15527-2004  (inclusive of materials) | pcs | 96 | Certificate of conformity and quality |
|  | Installation of collecting pipe made of ∅32 electric welded steel pipe (with 6 outlets - outlet ∅25 ) (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
|  | Installation of plastic sludge trap (dirt collector); ∅ 32, PN16 (inclusive of materials) | pcs | 30 | Certificate of conformity and quality |
| **Kindergarten 1B - heating system** | | | | |
|  | Heating device - installation of sectional aluminum radiators Sections = 14 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 12 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 13 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 8 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 5 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 3 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 40 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 87 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅32 х 2,9 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 5 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅ 25 х 2,3 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 156 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅20 х 1,9 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 171 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅32 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 5 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅25 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 156 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅20 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 171 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve ∅ 32, SDR6 PN16 ГОСТ 32415-2013 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass radiator valve ∅15 PN10 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 46 | Certificate of conformity and quality |
|  | Installation of radiator accessories (radiator hanging hook 2 pcs, radiator headings 4 pcs, bleeder screw 1 pc, ∅15 connector - outer thread - 2 pcs for each set) (inclusive of materials) | set | 23 | Certificate of conformity and quality |
| **Control junction 1, 2, 3, 4, 5** | | | | |
|  | Installation of steel electric welded pipe ∅ 108 x 4 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 6 | Certificate of conformity and quality |
|  | Galvanized steel pipe for hot water supply ∅80 x 3,5 mm ГОСТ 3262-75 (with piping components - flare joint, elbow pipe etc.) (inclusive of materials) | metre | 6 | Certificate of conformity and quality |
|  | Galvanized steel pipe for hot water supply ∅50 x 3 mm ГОСТ 3262-75 (with piping components - flare joint, elbow pipe etc.) (inclusive of materials) | metre | 6 | Certificate of conformity and quality |
|  | Galvanized steel pipe for hot water supply ∅40 x 3.0 mm ГОСТ 3262-75 (with piping components - flare joint, elbow pipe etc.) (inclusive of materials) | metre | 3 | Certificate of conformity and quality |
|  | Galvanized steel pipe for hot water supply ∅20 x 2,5 mm ГОСТ 3262-75 (with piping components - flare joint, elbow pipe etc.) (inclusive of materials) | metre | 2 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve (with piping components - flare joint, elbow pipe etc.) ∅ 100, PN16 / ЛС59-1 ГОСТ 15527-2004. (inclusive of materials) | pcs | 8 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve. (inclusive of materials); (with piping components - flare joint, elbow pipe etc.) ∅ 80, PN16 / ЛС59-1 ГОСТ 15527-2004 | pcs | 4 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve ∅ 50, PN16 / ЛС59-1 ГОСТ 15527-2004 (with piping components - flare joint, elbow pipe etc.) (inclusive of materials); | pcs | 3 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve∅ 40, (with piping components - flare joint, elbow pipe etc.) PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials); | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve ∅ 32 (with piping components - flare joint, elbow pipe etc.) PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve ∅ 25, (with piping components - flare joint, elbow pipe etc.) PN10 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials); | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve ∅ 20, (with piping components - flare joint, elbow pipe etc.) PN10 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials); | pcs | 4 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve ∅ 15, (with piping components - flare joint, elbow pipe etc.) PN10 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials); | pcs | 4 | Certificate of conformity and quality |
|  | Installation of cast iron mud trap (dirt collector) ∅100, (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) PN16 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Installation of cast iron mud trap (dirt collector) ∅80, (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) PN16 (inclusive of materials) | pcs | 1 | Certificate of conformity and quality |
|  | Installation of cast iron mud trap (dirt collector) ∅50, (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) PN16 (inclusive of materials) | pcs | 1 | Certificate of conformity and quality |
|  | Installation of cast iron mud trap (dirt collector) ∅40, (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) PN16 (inclusive of materials) | pcs | 1 | Certificate of conformity and quality |
|  | Installation of plastic mud trap (dirt collector) ∅25, (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) PN10 (inclusive of materials) | pcs | 1 | Certificate of conformity and quality |
|  | Installation of pressure regulating industrial pressure gauge (monometer) D - Ø100; thread - m 20 x 1,5; accuracy class - 2,5; 16 bar; İP-40; vibration resistant ГОСТ 2405-88 0-6 bar, (inclusive of materials) | pcs | 20 | Certificate of conformity and quality |
|  | Installation of technical temperature gauge 0-120 ºC, Alltan joint, Brass, Bi-Metallic, Ø 100 mm PN16 (inclusive of materials) | pcs | 10 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅159 х 4,0 / l=2000 mm (outlet - 40 x 3 mm -1 pc., 57 x 3,0 mm - 1 pc, 108 x 3 mm - 1 pc) (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 108 x 4 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 6 | Certificate of conformity and quality |
| **Heating network general lay out** | | | | |
|  | Compensator - compensatory movement L 30 mm (-20 ... + 10 mm) (flanged, on pipe) ∅ 100 - stainless steel PN16 (bolt, nut, padding, etc.) Flex pipe - x5CrNi; Flange - St37; Flex pipe length = 190 mm ОФН -16-100 ГОСТ 32935-2014 (inclusive of materials) | pcs | 24 | Certificate of conformity and quality |
|  | Compensator - compensatory movement L 30 mm (-20 ... + 10 mm) (flanged, on pipe) ∅ 65 - stainless steel PN16 (bolt, nut, padding, etc.) Flex pipe - x5CrNi; Flange - St37; Flex pipe length = 175 mm ОФН -16-65 ГОСТ 32935-2014 (inclusive of materials) | pcs | 8 | Certificate of conformity and quality |
|  | Compensator - compensatory movement L 60 mm (-40 ... + 20 mm) (flanged, on pipe) ∅ 32 - stainless steel PN16 (bolt, nut, padding, etc.) Flex pipe - x5CrNi; Flange - St37; Flex pipe length = 120 mm ОФН -16-32 ГОСТ 32935-2014 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Compensator - compensatory movement L 60 mm (-40 ... + 20 mm) (flanged, on pipe) ∅ 20 - stainless steel PN16 (bolt, nut, padding, etc.) Flex pipe - x5CrNi; Flange - St37; Flex pipe length = 120 mm ОФН -16-20 ГОСТ 32935-2014 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Electric welded steel pipes ∅ 108 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 640 | Certificate of conformity and quality |
|  | Galvanized steel pipes designed for water and gas supply ∅100 х 4.0 ГОСТ 3262-75 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 320 | Certificate of conformity and quality |
|  | Galvanized steel pipes designed for water and gas supply ∅65 х 3.2 ГОСТ 3262-75 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 320 | Certificate of conformity and quality |
|  | Galvanized steel pipes designed for water and gas supply ∅32 х 2.8 ГОСТ 3262-75 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.)  (inclusive of materials) | metre | 160 | Certificate of conformity and quality |
|  | Galvanized steel pipes designed for water and gas supply ∅20 х 2.5 ГОСТ 3262-75 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 160 | Certificate of conformity and quality |
| **External supply lines** | | | | |
|  | Installation of steel electric welded pipe ∅ 108 x 4 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 72 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 76 x 3 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 639 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅100 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 72 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅70 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 639 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve ∅ 100, PN16 / ЛС59-1 ГОСТ 15527-2004 (with piping components - flare joint, elbow pipe etc.) (inclusive of materials); | pcs | 4 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve; (with piping components - flare joint, elbow pipe etc.) ∅ 70, PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 12 | Certificate of conformity and quality |
|  | Installation of brass shut - off and release valve; (with piping components - flare joint, elbow pipe etc.) ∅ 32, PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of plastic shut - off and release valve ∅25, SDR6 PN10 ГОСТ 32415-2013 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Heating device - installation of sectional aluminum radiators Sections = 10 h = 577 mm ГОСТ 31311-2005 / ГОСТ 8617 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass radiator valve ∅15 SDR6 PN10 ГОСТ 32415-2013 (inclusive of materials) | pcs | 4 | Certificate of conformity and quality |
|  | Installation of radiator accessories (radiator hanging hook 2 pcs, radiator headings 4 pcs, bleeder screw 1 pc, ∅15 connector - outer thread - 2 pcs for each set) (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of pressure resistant - PPR (polypropylene random copolymer) - plastic water pipe with foil SDR6 ∅20 х 1,9 PN25 ГОСТ 32415-2013 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 130 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅20 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 130 | Certificate of conformity and quality |
| **Air release chamber** | | | | |
|  | Installation of steel electric welded pipe ∅ 40 x 3,0 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 56 | Certificate of conformity and quality |
|  | Installation of steel electric welded pipe ∅ 32 x 2,2 mm, II ГОСТ 10704-91 / B-Ст3сп ГОСТ 10705-80 (with piping components - coupling, t-shaped pipe joint, elbow pipe 90º, clamp, etc.) (inclusive of materials) | metre | 4 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅40 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 56 | Certificate of conformity and quality |
|  | Installation of thermal insulation for ∅32 pipes 13 mm PEF (foamed polyethylene) ГОСТ Р 56729-2015 (EN 14313: 2009) (inclusive of materials) | metre | 4 | Certificate of conformity and quality |
|  | Installation of brass radiator valve (inclusive of materials) ∅25 PN10 / ЛС59-1 ГОСТ 15527-2004 | pcs | 8 | Certificate of conformity and quality |
|  | Installation of brass trizonal valve ∅32 PN16 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass automatic air release valve ∅15 PN10 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
|  | Installation of brass water bleeder ∅15 PN10 / ЛС59-1 ГОСТ 15527-2004 (inclusive of materials) | pcs | 2 | Certificate of conformity and quality |
| **Mechanical work** | | | | |
|  | Wall chasing to make trench for heating system pipelines (inclusive of materials) | running metre | 1400 |  |
|  | Grouting of wall trenches for heating system pipelines (inclusive of materials) | running metre | 1400 |  |

* **Technical requirements and the scope of work related to the installation of heating systems in the multi-storeyed residential building with a kindergarten on the ground floor on the balance sheet of the "Denizchi" Construction Housing Cooperative under "ACS" CJSC :**
* **The requirements of the Project documents shall be observed during the installation of heating systems in the buildings.**
* **It is required to provide the quality certificate, certificate of conformity and information on the manufacturer and information on technical parameters for the materials used.**
* **Delivery time for the works shall be specified.**
* **A license (for the construction of utilities and networks) shall be submitted for construction works.**
* **For the performance of the works, the entity shall provide details of the trial and maintenance spaces, technical capacities of the entity and appropriate permits and experience of the personnel.**
* **The personnel of the construction organization shall hold certificates as specified in the scope of work.**
* **Information on official employees of the construction organization shall be provided.**
* **The specialized organization shall have at least 3 years work experience and submit contracts for the installation of the heating system concluded within last 3 years.**
* **While performing construction works, safety rules of ACS CJSC and construction safety rules shall be complied with.**

For technical questions please contact :

Elvin Aliyev - Head of Technical Maintenance Division of “Denizchi repair and construction” LLC

Telephone no. : +99450 2286364

**E-mail:** [**elvin.aliyev@asco.az**](mailto:elvin.alıyev@asco.az)

**For technical questions please contact :**

Javid Eminov, Engineer of Construction and Repair department

Telephone no. : +99450 2740251

E-mail: cavid.eminov@acsc.az

Due diligence shall be performed in accordance with the Procurement Guidelines of ASCO prior to the conclusion of the purchase agreement with the winner of the bidding.

The company shall enter through this link http: //asco.az/sirket/satinalmalar/podratcilarin-elektron-muraciet-formasi// to complete the special form or submit the following documents:

* Articles of Association of the company (all amendments and changes including)
* An extract from state registry of commercial legal entities (such extract to be issued not later than last 1 month)
* Information on the founder in case if the founder of the company is a legal entity
* Certificate of Tax Payer`s Identification Number
* Audited accounting balance sheet or tax declaration (depending on the taxation system) / reference issued by taxation bodies on non-existence of debts for tax
* Identification card of the legal representative
* Licenses necessary for provision of the relevant services / works (if any)

No agreement of purchase shall be concluded with the company which did not present the above-mentioned documents or failed to be assessed positively as a result of the due diligence performed and shall be excluded from the bidding !