Approved by the order of the Chairman of "Azerbaijan Caspian Shipping Closed Joint Stock Company dated 1st of December 2016No. 216.



**AZERBAIJAN CASPIAN SHIPPING CLOSED JOINT STOCK COMPANY IS ANNOUNCING OPEN BIDDING FOR THE PROCUREMENT OF HOSES OF VARIOUS PURPOSE REQUIRED FOR STRUCTURAL DEPARTMENTS**

 **B I D D I N G No. AM075 / 2024**

|  |  |
| --- | --- |
|  | **Submission documentation required for participation in the bidding :*** Application for participation in the bidding (template has been attached hereto) ;
* Bank evidence as a proof of participation fee ;
* Bidding offer :
* Bank document confirming financial condition of the consignor within the last year (or within the period of operation if less than one year) ;
* Statement issued by the relevant tax authorities on the absence of expired commitments associated with taxes and other compulsory payments and failure of obligations set forth in the Tax Code of the Republic of Azerbaijan for the last one year (excluding the period of suspension).

At the initial stage, application for participation in the bidding ( signed and stamped ) and bank evidence proving payment of participation fee (excluding bidding offer) shall be submitted in English, Russian or in Azerbaijani to the official address of Azerbaijan Caspian Shipping CJSC (hereinafter referred to as "ASCO" or "Procuring Organization") through email address of contact person in charge by **17.00** (Baku time) on **june 07, 2024**. Whereas, other necessary documents shall be submitted as enclosed in the bidding offer envelope.   Description (list) of goods, works or services has been attached hereto.  |
|  | **The participation fee and Collection of General Terms and Conditions:*** Any participant (bidder), who desires to participate in the bidding, shall pay for participation fee stated below (the payment order shall necessarily state the name of the organization holding open bidding and the subject of the bidding) and shall submit the evidence as a proof of payment to ASCO not later than the date stipulated in section one. All participants (bidders), who have fulfilled these requirements, may obtain General Terms and Conditions relating to the procurement subject from contact person in charge by the date envisaged in section IV of this announcement at any time from 09.00 till 18.00 in any business day of a week.
* Participation fee amount (VAT exclusive): 150 Azn.
* The participation fee may be paid in AZN or equivalent amount thereof in USD or EURO.
* ***Account No. :***

|  |  |  |
| --- | --- | --- |
| AZN  | USD | EURO  |
| Name : The International Bank of Azerbaijan ABB- Customer Service DepartmentCode : 805250TAX ID : 9900001881Correspondent account : AZ03NABZ01350100000000002944SWIFT : IBAZAZ2XBeneficiary: AZARB.XAZAR DANIZ GAMICILIYI QSCTAX ID : 1701579951Account No. (AZN) : AZ36IBAZ38050019441115341120 | Intermediary Bank : Citibank N.Y, New YorkAcc.36083186, SWIFT: CITIUS33Beneficiary Bank : The International Bank of AzerbaijanIBA- Customer Service DepartmentSWIFT : IBAZAZ2X Nizami str., 67Beneficiary : AZARB.XAZAR DANIZ GAMICILIYI QSCTAX ID : 1701579951Account No. : AZ26IBAZ38150018401115341120 | Intermediary Bank : Commerzbank AG, Frankfurt am MainSWIFT : COBADEFFACC # 400 88 660 3001Beneficiary Bank : The International Bank of Azerbaijan,IBA-Premier Customer ServiceSWIFT : IBAZAZ2X Nizami str., 67Beneficiary : Azerbaijan Caspian Shipping CJSCTAX ID : 1701579951Account No. : AZ06IBAZ38150019781115341120 |

* **Except for circumstances where the bidding is cancelled by ASCO, participation fee shall in no case be refunded !**
 |
|  |  **Security for a bidding offer :** * The bank guarantee is required in the amount of at least 1 (one) % of the bidding offer price. A bank guarantee sample shall be specified in the General Terms and Conditions.
* Bank guarantees shall be submitted as enclosed in the bidding offer envelope along with the bidding offer. Otherwise, the Purchasing Organization shall reserve the right to reject such offer.
* The financial institution that issued the guarantee should be acknowledged in the Republic of Azerbaijan and / or international financial transactions. The purchasing organization shall reserve the right not to accept and reject any unreliable bank guarantee.
* Persons wishing to participate in the bidding and intending to submit another type of warranty (letter of credit, securities, transfer of funds to the special banking account set forth by the Procuring Organization in the bidding documents, deposit and other financial assets) shall request and obtain a consent from ASCO through the contact person reflected in the announcement on the acceptability of such type of warranty.
* Contract performance bond is required in the amount of 5 (five) % of the purchase price.
* For the current procurement operation, the Procuring Organization is expected to make payment only after the goods have been delivered to the warehouse, no advance payment has been intended.

**Contract Performance Term :** * The goods will be purchased on an as needed basis. It is required that the contract of purchase be fulfilled within 5 (five) calendar days upon receipt of the formal order (request) placed by ASCO.
 |
|  | **Final deadline date and time for submission of the bidding offer :*** All participants, which have submitted their application for participation in the bidding and bank evidence as a proof of payment of participation fee by the date and time stipulated in section one, and shall submit their bidding offer (one original and two copies) enclosed in sealed envelope to ASCO by **17.00** Baku time on **june 13, 2024** All bidding offer envelopes submitted after above-mentioned date and time shall be returned unopened.
 |
|  | **Address of the procuring company :**The Azerbaijan Republic, Baku city, AZ1029 (postcode), 2 Neftchilar Avenue, Procurement Committee of ASCO. **Contact person in charge:**Rahim AbbasovProcurement specialist at the Procurement Department of ASCOTelephone No. : **+99450 2740277**Email address: rahim.abbasov@asco.az, tender@asco.az**Contact person on legal issues :**Landline No.: +994 12 4043700 (ext: 1262)Email address: tender@asco.az |
|  | **Date and time assigned for the opening of bidding offer envelopes:**Opening of the envelopes shall take place on **june 14, 2024,** at **14.00** Baku time in the address stated in section V of the announcement. Persons wishing to participate in the opening of the envelopes shall submit a document confirming their permission to participate (the relevant power of attorney from the participating legal entity or natural person) and the ID card at least half an hour before the commencement of the bidding. |
|  | **Information on the winner of the bidding :**Information on the winner of the bidding will be posted in the "Announcements" section of the ASCO official website.  |

(On the participant`s letter head)

APPLICATION FOR PARTICIPATION IN

THE OPEN BIDDING

\_\_\_\_\_\_\_\_\_\_\_ city “\_\_”\_\_\_\_\_\_\_20\_

\_\_\_\_\_\_\_\_\_\_\_№

To the attention of the Chairman of ASCO Procurement Committee

Mr Jabrail Mahmudlu

We, hereby confirm the intention of [ to state full name of the participant ] to participate in the open bidding No. [ bidding No. shall be inserted by participant ] announced by ASCO in respect of procurement of "\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_" .

Moreover, we confirm that no winding - up or bankruptcy proceeding is being performed or there is no circumstance of cessation of activities or any other circumstance that may impede participation of [ to state full name of the participant ] in the stated bidding.

In addition, we warrant that [ to state full name of the participant ] is not an affiliate of ASCO.

Below mentioned contact details are available to respond to any question that may emerge in relation to the documents submitted and other issues :

* Contact person in charge :
* Position of the contact person :
* Telephone No. :
* E-mail:

Attachment :

1. Original of the bank evidence as a proof of payment of participation fee – \_\_ page(s).

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(initials of the authorized person) (signature of the authorized person)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 (position of the authorized person)

 **STAMP HERE**

 **LIST OF THE GOODS:**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| № | Nomination of goods | General description | Quantity | Measurement unit | Requisition | Department name | Certification requirement |
| 1 | Fuel hose Б (I) - 16 - 75 - 100  | Fuel hose Б(I) - 16 - 75 - 100 - У ГОСТ 18698-79 (reinforced textile) | 200 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 2 | Transparent water hose (PVC) ВГ - II - Ø 16 x 20 mm | Transparent water hose (PVC) ВГ - II - Ø 16 x 20 mm ТУ 2247 - 001 - 98251521 - 2014 | 150 | m | 10088532 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 3 | Water hose - В(II) - 10 - 38 - 55 - У ГОСТ 18698-79 | Water hose - В(II) - 10 - 38 - 55 - У ГОСТ 18698-79 | 200 | m | 10091390 | The Marine Transportation Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 4 | Air hose Ø 16 mm, 10 bar, ISO2398 | Air hose Ø 16 mm equipped with plastic internal side 10 bar ISO2398 | 100 | m | 10091390 | The Marine Transportation Fleet | Conformity and quality certificate |
| 5 | Water hose - В(II) - 6,3 - 32 - 43 - У (equipped with cotton wire) | Water hose - В(II) - 6,3 - 32 - 43 - У ГОСТ 18698-79 (armored with cotton wire) | 1 000 | m | 10091390 | The Marine Transportation Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 6 | Water hose - В(II) - 16 - 50 - 75 - У (armored with cotton wire) | Water hose - В(II) - 16 - 50 - 75 - У ГОСТ 18698-79 (armored with cotton wire) | 300 | m | 10091390 | The Marine Transportation Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 7 | Fuel hose Ø 75 mm, 16 bar. L - 30 m | Fuel hose - internal Ø 75 mm, external Ø 89 mm, 16 bar. L-30 m, with cam lock joint at one end Ø 75 mm, 20 bar, with universal joint at another end Ø 75 mm | 5 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 8 | Sandblasting hose 1 1/4" Ø 32 x 48 mm, 12 - 36 bar | Sand blasting device hose 1 1 / 4" 32 X 4 8 mm, 12 - 36 bar, ISO 3861:2021, ISO1307 | 600 | m | 10091448 | Bibiheybat Ship Repair Yard | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 9 | Liquefied gas hose 1/4" Ø 6 x 14 mm, 20 bar | Liquefied gas hose 1/4" internal 6 mm external 14 mm 20 bar DIN 8541 | 1 500 | m | 10091448 | Bibiheybat Ship Repair Yard | Conformity and quality certificate |
| 10 | Oxygen hose 1/4" Ø 6 x 14 mm, 20 bar | Oxygen hose 1/4" internal 6 mm external 14 mm 20 bar DIN 8541 | 1 500 | m | 10091448 | Bibiheybat Ship Repair Yard | Conformity and quality certificate |
| 11 | Fecal hose, 75 mm, 16 bar. L - 30 m 2 cam locks | Fecal hose, internal Ø 75 mm, external Ø 89 mm 16 bar. L - 30 m both ends equipped with cam lock coupling. Ø 75 mm, 20 bar | 4 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 12 | Universal joint for camlock 100 mm (female)  | Universal joint for camlock 100 mm (female) | 7 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 13 | Universal joint for camlock 100 mm (male)  | Universal joint for camlock 100 mm (male) | 7 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 14 | WECO connector (with internal thread) 4" | WECO connector (with internal thread) 4" | 8 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 15 | Fuel hose Ø 100 mm; 16 bar, with metallic frame | Fuel hose - Ø -100 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1361 | 80 | m | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 16 | Mud hose Ø 100 mm; 16 bar metal frame | Mud hose - Ø -50 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1364 | 80 | m | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 17 | Benzol hose Ø 100 mm; 16 bar, with metallic frame | Benzol hose - Ø - 100 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1365 | 80 | m | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 18 | Cement hose Ø 100 mm; 16 bar, with metallic frame | Cement hose - Ø - 100 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1366 | 120 | m | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 19 | Water hose - Ø 100 mm; 16 bar metal frame | Water hose - Ø - 100 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1371 | 80 | m | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 20 | Joint (Weko) Hummer internal thread Ø 100 mm | Hose nozzle with internal threading (Weko) Hummer Ø - 100 mm FIG. 10000: 4 NPT API 16 A-ISO14693 | 7 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 21 | TODO connector (with internal thread) 4" | WECO connector (with internal thread) 4" | 3 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 22 | Todo Matik joint Ø 75 mm, 20 bar, internal thread | Todo Matik joint Ø - 75 mm 20 bar internal thread (Female) - NATO STANAG 3756 standard | 7 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 23 | Water hose 75 mm, 16 bar (1 Weco 4 ``joint) | Water hose 75 mm, 16 bar (with Weco 4``(Ø100mm) joint at one end) | 40 | m | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 24 | Fuel hose Ø 50 mm; 16 bar, with metallic frame | Fuel hose - Ø -50 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1361 | 120 | m | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 25 | Joint (Weko) Hummer internal thread Ø 75 mm | Hose nozzle with internal threading (Weko) Hummer Ø - 75 mm FIG. 10000: 4 NPT API 16 A-ISO14693 | 4 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 26 | Todo Matik joint Ø 100 mm, 20 bar, with external thread | Todo Matik joint Ø - 100 mm 20 bar internal thread (Female) - NATO STANAG 3756 standard | 2 | p c s | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 27 | Fecal hose - Ø 50 mm; 16 bar metal frame | Fecal hose - Ø -50 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1368 | 100 | m | 10092697 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 28 | Air hose Ø 16 mm, 10 bar, ISO2398 | Air hose Ø 16 mm equipped with plastic internal side 10 bar ISO2398 | 100 | m | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 29 | Durite hose Ø 42 mm, 10 bar ГОСТ 18698 - 79 | Durite hose internal diameter Ø 42 mm, 10 bar ГОСТ 18698 - 79 | 40 | m | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 30 | Durite hose Ø 25 mm, 10 bar ГОСТ 18698 - 79 | Durite hose Ø 25 mm, 10 bar ГОСТ 18698 - 79 | 50 | m | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 31 | Water hose (black) 20 х 30 - 1 ГОСТ 10362 - 2017 | Water hose (black) 20 х 30 - 1 ГОСТ 10362 - 2017 | 100 | m | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 32 | Transparent water hose (PVC) ВГ - II - Ø 25 x 30 mm | Transparent water hose (PVC) ВГ - II - Ø 25 x 30 mm ТУ 2247 - 001 - 98251521 - 2014 | 40 | m | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 33 | Spiral equipped air hose 8 x 12 mm / 15 m, 8 bar | Spiral equipped air hose 8 x 12 mm / 15 m, 8 bar | 2 | p c s | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 34 | Water hose (rubber) Ø 15 mm 6 bar | Water hose (rubber) Ø 15 mm 6 bar | 250 | m | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 35 | High pressure hose 8/3" 15.2 m 310 bar | High pressure hose 1/4" 15.2 m 310 bar H73850 | 7 | p c s | 10092594 | Zykh Ship Repair and Construction Yard | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 36 | High pressure hose 1/4" 1.8 m 310 bar | High pressure hose 1/4" 1.8 m 310 bar H72506 | 10 | p c s | 10092594 | Zykh Ship Repair and Construction Yard | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 37 | Air hose 20 x 29 - 2,5 B | Air hose 20 x 29 - 2,5 B ГОСТ 10362 - 2017 | 300 | m | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 38 | Sandblaster hose 32 x 8 mm, 12 - 36 bar | Sandblaster hose 32 x 8 mm, 12 - 36 bar | 300 | m | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 39 | Hose 7.5 m (for VAF-300 fan) | Hose 7.5 m (for VAF-300 fan) | 5 | p c s | 10092594 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 40 | Air hose Ø 16 mm, 10 bar, ISO2398a | Air hose Ø 16 mm equipped with plastic internal side 10 bar ISO2398 | 800 | m | 10091448 | Bibiheybat Ship Repair Yard | Conformity and quality certificate |
| 41 | Durite hose Ø 38 mm 10 bar ГОСТ 18698 - 79 | Durite hose Ø 38 mm 10 bar ГОСТ 18698 - 79 | 510 | m | 10091448 | Bibiheybat Ship Repair Yard | Conformity and quality certificate |
| 42 | Durite hose Ø 25 mm, 10 bar ГОСТ 18698 - 79 | Durite hose Ø 25 mm, 10 bar ГОСТ 18698 - 79 | 50 | m | 10088185 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 43 | Durite hose Ø 38 mm 10 bar ГОСТ 18698 - 79 | Durite hose Ø 38 mm 10 bar ГОСТ 18698 - 79 | 10 | m | 10088185 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 44 | Durite hose internal Ø 42 mm, 10 bar ГОСТ 18698 - 79 | Durite hose internal diameter Ø 42 mm, 10 bar ГОСТ 18698 - 79 | 20 | m | 10088185 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 45 | Durite hose internal Ø 48 mm, 10 bar ГОСТ 18698 - 79 | Durite hose internal diameter Ø 48 mm, 10 bar ГОСТ 18698 - 79 | 20 | m | 10088185 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 46 | Water hose WDH1-50/2” - Ø 50.8 - 62,10 bar | Water hose WDH1 - 50/2”- Ø 50.8 - 62 (ISO 1402) 10 bar burst limit 30 bar | 20 | m | 10088185 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 47 | Fuel hose Ø 100 mm; 16 bar, with metallic frame | Fuel hose - Ø -100 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1361 | 200 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 48 | Mud hose Ø 100 mm; 16 bar metal frame | Mud hose - Ø -50 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1364 | 150 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 49 | Benzol hose Ø 100 mm; 16 bar, with metallic frame | Benzol hose - Ø - 100 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1365 | 150 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 50 | Fecal hose - В(II) - 16 - 75 - 100  | Fecal hose Б(I) - 16 - 75 - 100 - У ГОСТ 18698 - 79 (reinforced textile) | 100 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 51 | Cement hose Ø 100 mm; 16 bar, with metallic frame | Cement hose - Ø - 100 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1366 | 150 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 52 | Fuel hose Ø 50 mm; 16 bar, with metallic frame | Fuel hose - Ø -50 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1361 | 250 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 53 | Water hose 75 mm, 16 bar (1 Weco 4 ``joint) | Water hose 75 mm, 16 bar (with Weco 4``(Ø100mm) joint at one end) | 100 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 54 | Underfloor hose Ø 50 mm with joints at both ends, 10 bar | Underfloor water hose, Hose external Ø 65 mm, internal Ø 50 mm, 10bar. Both ends equipped with universal joint. Joint external Ø 126 mm, internal Ø41 mm | 100 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 55 | Water hose 75 mm, 16 bar (1 Weco 4 ``joint) | Water hose 75 mm, 16 bar (with Weco 4``(Ø100mm) joint at one end) | 150 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 56 | Household water hose Ø 50 mm, 2 joints 10 bar | Domestic water hose, external Ø 65 mm, internal Ø 50 mm, 10 bar. Equipped with universal coupling at both ends Coupling: external Ø 162 mm, internal Ø 37 mm. | 100 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 57 | Fuel hose Ø 50 mm; 16 bar, with metallic frame | Fuel hose - Ø -50 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1361 | 200 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 58 | Water hose WDH1-50/2” - Ø 50.8 - 62,10 bar | Water hose WDH1 - 50/2”- Ø 50.8 - 62 (ISO 1402) 10 bar burst limit 30 bar | 150 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 59 | Water hose WDH1 - 32/1 - 1/4" Ø 31,8 - 42,10 bar | Water hose WDH1 - 32/ 1 - 1/4" - Ø 31,8 - 42 (ISO 1402) 10 bar burst limit 30 bar | 100 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 60 | Oil hose Б(I) - 16 - 75 - 100 - У (reinforced textile) | Oil hose Б(I) - 16 - 75 - 100 - У ГОСТ 18698-79 (reinforced textile) | 200 | m | 10088532 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 61 | Durite hose Ø 25 mm, 10 bar ГОСТ 18698 - 79 | Durite hose Ø 25 mm, 10 bar ГОСТ 18698 - 79 | 96 | m | 10088532 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 62 | Durite hose Ø 38 mm 10 bar ГОСТ 18698 - 79 | Durite hose Ø 38 mm 10 bar ГОСТ 18698 - 79 | 19 | m | 10088532 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 63 | Durite hose internal Ø 42 mm, 10 bar ГОСТ 18698 - 79 | Durite hose internal diameter Ø 42 mm, 10 bar ГОСТ 18698 - 79 | 38 | m | 10088532 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 64 | Durite hose internal Ø 48 mm, 10 bar ГОСТ 18698 - 79 | Durite hose internal diameter Ø 48 mm, 10 bar ГОСТ 18698 - 79 | 38 | m | 10088532 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 65 | Water hose - В(II) - 6,3 - 25 - 36 - У (equipped with cotton wire) | Water hose - В(II) - 6,3 - 25 - 36 - У ГОСТ 18698-79 (armored with cotton wire) | 400 | m | 10091390 | The Marine Transportation Fleet | Conformity and quality certificate |
| 66 | Durite hose Ø 25 mm, 10 bar ГОСТ 18698 - 79 | Durite hose Ø 25 mm, 10 bar ГОСТ 18698 - 79 | 600 | m | 10091448 | Bibiheybat Ship Repair Yard | Conformity and quality certificate |
| 67 | Air hose internal 16mm, external 26 mm 10 bar | Air hose, 5/8" internal, 16 mm, external - 26 mm 10 bar. burst 30 bar ISO2398 | 32 | m | 10091448 | Bibiheybat Ship Repair Yard | Conformity and quality certificate |
| 68 | Air hose internal 8 mm, external 9.5 mm 10 bar | Air hose, 5/16" internal, 8 mm, external - 9.5 mm 10 bar. burst 30 bar ISO2398 | 500 | m | 10091448 | Bibiheybat Ship Repair Yard | Conformity and quality certificate |
| On general created requisitions |
| 1 | Durite hose internal dia. Ø 219 mm 10 bar, L = 300 mm ГОСТ 18698 - 79 | Durite hose internal dia. Ø 219 mm 10 bar, L = 300 mm (Heat-resistant) ГОСТ 18698 - 79 | 8 | p c s | 10094845 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 2 | Fecal hose WDH1-50/2” - Ø 50.8 - 62,10 bar | Fecal hose WDH1 - 50/2”- Ø 50.8 - 62 (ISO 1402) 10 bar burst limit 30 bar | 20 | m | 10095654 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 3 | Water hose Ø - 15 mm, 6 bar, 30 m | Water hose Ø - 15 mm, 6 bar, 30 m | 1 | p c s | 10087378 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 4 | Durite hose internal Ø 114 mm, 10 bar ГОСТ 18698 - 79 | Durite hose internal Ø 114 mm, 10 bar ГОСТ 18698 - 79 | 2 | m | 10093107 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 5 | Fecal hose WDH1-50/2” - Ø 50.8 - 62,10 bar, 40 m | Fecal hose WDH1 - 50/2”- Ø 50.8 - 62 (ISO 1402) 10 bar burst limit 30 bar, 40 m | 2 | p c s | 10093282 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 6 | Cement hose Ø 101,16 bar, OSDH 3100, EN 1764 | Cement hose - Ø - 101 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; OSDH 3100, EN - 1764 | 50 | m | 10093282 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 7 | Underfloor hose 75 mm, 16 bar, L - 40 | Bilge water hose, internal Ø 75 mm, external Ø 89 mm, 16 bar. L - 40 m, complete with camlock coupling at both ends. Ø 75 mm, 20 bar | 1 | p c s | 10094254 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 8 | Pressure resistant air hose Ø 70 mm; 20 Bar | Pressure resistant air hose Ø 70 mm; 20 Bar | 25 | m | 10094279 | Bibiheybat Ship Repair Yard | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 9 | Bilge water hose В - 2 - 50 - 12 ГОСТ 5398 - 76 | Bilge water hose В - 2 - 50 - 12 ГОСТ 5398 - 76 | 15 | m | 10071669 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 10 | Fuel hose Б (I) - 16 - 50 - 68  | Fuel hose Б(I) - 16 - 50 - 68 - У ГОСТ 18698-79 (reinforced textile) | 30 | m | 10095438 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 11 | Cement hose Ø 100 mm; 16 bar, with metallic frame | Cement hose - Ø - 100 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1366 | 40 | m | 10092582 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 12 | Cement hose Ø 100 mm; 16 bar, with metallic frame | Cement hose - Ø - 100 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1366 | 40 | m | 10092582 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 13 | Fuel hose Ø 75 mm, 16 bar. L - 30 m | Fuel hose - internal Ø 75 mm, external Ø 89 mm, 16 bar. L - 30 m, with cam lock joint at one end Ø 75 mm, 20 bar, with universal joint at another end Ø 75 mm | 3 | p c s | 10093527 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 14 | Oil hose Б(I) - 16 - 50 - 68 - У (reinforced textile) | Oil hose Б(I) - 16 - 50 - 68 - У ГОСТ 18698-79 (reinforced textile) | 160 | m | 10093527 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 15 | Water hose 25 mm, 10 bars, 40 meters ISO 1402 | Water hose 1" 25 mm WDH1-25, 10 bars 40 meters collapse 30 bars (ISO 1402) | 20 | p c s | 10091702 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 16 | Oxygen hose Ø 8 mm (blue) 20 bar | Oxygen hose Ø 8 mm (blue color), external diameter Ø 13 mm, 20 bar | 30 | m | 10091111 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 17 | Propane hose Ø 8 mm (red color) 20 bar | Propane hose Ø 8 mm (red color) external diameter Ø 13 mm, 20 bar | 30 | m | 10091111 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 18 | Oxygen hose Ø 8 mm (blue) 20 bar | Oxygen hose Ø 8 mm (blue color), external diameter Ø 13 mm, 20 bar | 30 | m | 10091125 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 19 | Propane hose Ø 8 mm (red color) 20 bar | Propane hose Ø 8 mm (red color) external diameter Ø 13 mm, 20 bar | 30 | m | 10091125 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 20 | Oxygen hose Ø 8 mm (blue) 20 bar | Oxygen hose Ø 8 mm (blue color), external diameter Ø 13 mm, 20 bar | 30 | m | 10091113 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 21 | Propane hose Ø 8 mm (red color) 20 bar | Propane hose Ø 8 mm (red color) external diameter Ø 13 mm, 20 bar | 30 | m | 10091113 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 22 | Fecal hose - Ø 50 mm; 16 bar metal frame | Fecal hose - Ø -50 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1368 | 20 | m | 10087858 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 23 | Fecal hose - Ø 50 mm; 16 bar metal frame | Fecal hose - Ø -50 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1368 | 20 | m | 10087879 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 24 | Underfloor hose 50 mm.12 Б(I) - 16 - 50 - 68 - У | Underfloor hose Ø - 50 mm. 12 bar Б (I) - 16 - 50 - 68 - У ГОСТ 18698 - 79 (reinforced textile) | 20 | m | 10087879 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 25 | High pressure hose 100DN 19 LD | High pressure hose Hypress Water/3LAST 1000DN 19L 3/4-WP 1000 BAR/14500 PSI ISO1/1-2/5//Length 1000 mm. | 2 | p c s | 10086094 | ASCO | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 26 | Oil hose Б(I) - 16 - 50 - 68 - У (reinforced textile) | Oil hose Б(I) - 16 - 50 - 68 - У ГОСТ 18698-79 (reinforced textile) | 1 | m | 10094684 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 27 | Fecal hose Ø 75 mm, 20 bar, 20 m ISO 1402 | Fecal hose Ø 75 mm, 20 meters external Ø 89 mm, 20 bar burst 40 bar WDH1 - 76/3” 76.2 - 89 (ISO 1402) | 2 | p c s | 10094684 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 28 | Freon adding hose L = 1 m, 1/4", 40 bar | Freon adding hose: L = 1 m, 1/4" SAE x 1/4" SAE, 40 bar | 1 | p c s | 10094717 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 29 | Water hose (rubber) Ø 15 mm 6 bar | Water hose (rubber) Ø 15 mm 6 bar | 20 | m | 10088070 | Zykh Ship Repair and Construction Yard | Conformity and quality certificate |
| 30 | Oil hose Б(I) - 16 - 50 - 68 - У (reinforced textile) | Oil hose Б(I) - 16 - 50 - 68 - У ГОСТ 18698-79 (reinforced textile) | 40 | m | 10093921 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 31 | Fuel hose Ø 50 mm; 16 bar, with metallic frame | Fuel hose - Ø -50 mm; 16 bar reinforced synthetic cord with metallic frame + antistatic copper wire.; ISO 1307 EN1361 | 40 | m | 10093921 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 32 | Water hose - В(II) - 6,3 - 32 - 43 - У (equipped with cotton wire) | Water hose - В(II) - 6,3 - 32 - 43 - У ГОСТ 18698-79 (armored with cotton wire) | 30 | m | 10088263 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 33 | Durite hose internal dia. Ø 219 mm 10 bar, L = 300 mm ГОСТ 18698 - 79 | Durite hose internal dia. Ø 219 mm 10 bar, L = 300 mm (Heat-resistant) ГОСТ 18698 - 79 | 8 | p c s | 10092373 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 34 | Water hose - В(II) - 16 - 50 - 75 - У (armored with cotton wire) | Water hose - В(II) - 16 - 50 - 75 - У ГОСТ 18698-79 (armored with cotton wire) | 40 | m | 10086117 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 35 | Fecal hose - В(II) - 16 - 75 - 100  | Fecal hose B (I) - 16 - 75 - 100 - У ГОСТ 18698 - 79 (reinforced textile) | 20 | m | 10092359 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 36 | Water hose 25 mm, 10 bars, 40 meters ISO 1402 | Water hose 1" 25 mm WDH1-25, 10 bars 40 meters collapse 30 bars (ISO 1402) | 1 | p c s | 10092359 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 37 | Water hose (rubber) Ø 15 mm 6 bar | Water hose (rubber) Ø 15 mm 6 bar | 30 | m | 10085710 | The Caspian Sea Oil Fleet | Conformity and quality certificate |
| 38 | Hydraulic hose 2 m, ø 18 mm, M14 nut | Hydraulic hose L - 2 m, ø 18 mm, threaded-nut on both sides M14, S19, 250 bar | 2 | p c s | 10086234 | The Production Services Department | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 39 | Hydraulic hose 2 m, ø 18 mm, M19 nut | Hydraulic hose L - 2 m, ø 18 mm, threaded-nut on both sides M19, S19, 250 bar | 1 | p c s | 10086234 | The Production Services Department | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 40 | Hydraulic hose 2 m, ø 20 mm, M19 nut | Hydraulic hose L - 2 m, ø 20 mm, threaded-nut on both sides M19, S19, 250 bar | 1 | p c s | 10086234 | The Production Services Department | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 41 | Underfloor hose Ø 50 mm with joints at both ends, 10 bar | Underfloor water hose, Hose external Ø 65 mm, internal Ø 50 mm, 10bar. Both ends equipped with universal joint. Joint external Ø 126 mm, internal Ø41 mm | 50 | m | 10096778 | The Caspian Sea Oil Fleet | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |

*Note :* ***The hoses will not be delivered at a time, but within a year by lots. Payment will be made only on actual basis.***

 **For technical questions please contact :**

**Mahir Isayev**

**Tel: +99450 2921232**

**E-mail:** **Mahir.İsyaev@asco.az**

**Elnur Mukhtarov**

**Tel: +99450 3767279**

**E-mail:Elnur.muxtarov****@asco.az**

**Gulu Guliev**

**Tel: +99450 2207820**

**E-mail: Qulu.quliyev****@asco.az**

Due diligence shall be performed in accordance with the Procurement Guidelines of ASCO prior to the conclusion of the purchase agreement with the winner of the bidding.

 The company shall enter through this link http: //asco.az/sirket/satinalmalar/podratcilarin-elektron-muraciet-formasi// to complete the special form or submit the following documents:

* Articles of Association of the company (all amendments and changes including)
* An extract from state registry of commercial legal entities (such extract to be issued not later than last 1 month)
* Information on the founder in case if the founder of the company is a legal entity
* Certificate of Tax Payer`s Identification Number
* Audited accounting balance sheet or tax declaration (depending on the taxation system) / reference issued by taxation bodies on non-existence of debts for tax
* Identification card of the legal representative
* Licenses necessary for provision of the relevant services / works (if any)

No agreement of purchase shall be concluded with the company which did not present the above-mentioned documents or failed to be assessed positively as a result of the due diligence performed and shall be excluded from the bidding!